**LIST OF FIGURES**

|  |  |  |
| --- | --- | --- |
| **S NO.** | **NAME OF THE FIGURE** | **Page No** |
| 3.1 | BASIC CIRCUIT FOR A DC MOTOR OPERATION PRINCIPLE | 9 |
| 3.2 | EQUIVALENT CIRCUIT OF PERMANENT MAGNET DC MOTOR | 11 |
| 3.3 | FOUR QUADRANT OPERATION | 12 |
| 3.4 | TWO QUADRANT CONVERTER | 13 |
| 3.5 | SINGLE QUADRANT CONVERTER | 13 |
| 3.6 | BLOCK DIAGRAM OF A DC MOTOR SPEED CONTROLLER IN A CLOSED LOOP SYSTEM | 14 |
| 4.1 | FIRST ARDUINO BOARD, LATE 2005 | 22 |
| 4.2  4.3  4.4  4.5 | A SCREENSHOT OF THE ARDUINO IDE SHOWING THE “BLINK" PROGRAM, A SIMPLE BEGINNER PROGRAM.  BLINK LED USING SIMULINK  CONNECTING LED TO ARDUINO  SIMULINK BLOCKS FOR ARDUINO | 23  27  28  29 |
| 5.1 | FLOW CHART OF THE PROJECT | 32 |
| 5.2 | CIRCUIT DIAGRAM OF THE DRIVE | 33 |
| 5.3 | ARDUINO MEGA 2560 DEVELOPER BOARD | 34 |
| 5.4 | OPTOCOUPLER 4N35 | 40 |
| 5.5 | PIN DIAGRAM OF OPTOCOUPLER 4N35 | 41 |
| 5.6 | TRANSISTOR TIP41C | 42 |
| 5.7 | DC MOTOR WITH ENCODER WITH ITS REMOVABLE COVER | 43 |
| 5.8 | STATE DIAGRAM AND WAVEFORM | 45 |
| 5.9  5.10 | PIN DESCRIPTION OF ENCODER MOTOR  COMPLETE LAB SETUP OF DEVELOPED KIT | 46  50 |
| 5.11 | DEVELOPED H-BRIDGE DRIVE CONNECTED TO ARDUINO AND MOTOR | 50 |
| 6.1 | SIMULINK CODE FOR OPEN-LOOP CONTROL SYSTEM | 49 |
| 6.2 | DIRECTIONS AND ON/OFF CONTROLLER BLOCK | 50 |
| 6.3 | MOTOR DRIVER BLOCK | 50 |
| 6.4 | ENCODER BLOCK | 51 |
| 6.5 | TRIGGERED SUBSYSTEM IN ENCODER BLOCK | 52 |
| 6.6 | SIMULINK MODEL FOR CLOSED-LOOP CONTROL WITH VARIABLE INPUT | 53 |
| 6.7 | PID CONTROLLER SUBSYSTEM | 53 |
| 6.8 | SIMULINK MODEL FOR CLOSED LOOP CONTROL WITH FIXED INPUT | 54 |
| 7.1 | DEVELOPED KIT FOR SPEED CONTROL OF DC MOTOR USING H-BRIDGE CONTROLLER THROUGH SIMULINK | 55 |
| 7.2 | RESULT ANALYSIS FOR AN INPUT FROM SIMULINK CONSTANT SOURCE BLOCK | 56 |
| 7.3 | RESULT ANALYSIS FOR AN INPUT FROM POTENTIOMETER | 57 |
| 7.4 | CLOSED LOOP CONTROL WITH P CONTROLLER | 58 |
| 7.5 | CLOSED LOOP CONTROL WITH PI CONTROLLER | 59 |
| 7.6 | CLOSED LOOP CONTROL WITH PID CONTROLLER | 60 |
| 7.7 | FORWARD DIRECTION OF DC MOTOR | 61 |
| 7.8 | FORWARD DIRECTION OF DC MOTOR | 61 |
|  |  |  |